(kicad_pcb (version 20241229) (generator "resinimport") (generator_version "1.0")
  (general (thickness 11.3792) (legacy_teardrops no))
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user "B.Fabrication")
    (49 "F.Fab" user "F.Fabrication")
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0.0)
    (allow_soldermask_bridges_in_footprints no)
    (stackup
      (layer "F.Cu"
        (type "copper")
        (thickness 0.03556)
      )
      (layer "dielectric 1"
        (type "core")
        (thickness 0.32004)
        (material "FR-4")
        (epsilon_r 4.8)
      )
      (layer "B.Cu"
        (type "copper")
        (thickness 0.03556)
      )
      (layer "dielectric 2"
        (type "core")
        (thickness 0.32004)
        (material "FR-4")
        (epsilon_r 4.8)
      )
    )
    (pcbplotparams
      (layerselection 0x0000172080000001)
      (plot_on_all_layers_selection 0x0000000000000000)
    )
  )
  (net 0 "")
  (net 1 "D_N")
  (net 2 "NetJ1_6")
  (net 3 "NetJ1_4")
  (net 4 "D_P")
  (net 5 "NetJ1_1")
  (net 6 "NetCN1_1")
  (net 7 "NetLED2_C")
  (net 8 "NetLED1_C")
  (net 9 "NetCN1_3")
  (net 10 "NetCN1_2")
  (net 11 "MISO")
  (net 12 "VIN")
  (net 13 "VCC5V")
  (net 14 "GND")
  (net_class "All Nets" ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6)
    (uvia_drill 0.3)
  )
  (footprint "HDR1X3"
    (layer "F.Cu")
    (at 150.50787 113.099044 180.0)
    (property "Reference" "J2" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Header, 3-Pin" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "HDR1X3" (at 0 0 0) (layer "F.Fab"))
    (pad "2" smd rect (at 4.879594 15.246096 270.0) (size 0.889 0.69977) (layers "F.Cu" "F.Paste" "F.Mask") (net 9 "NetCN1_3"))
    (pad "2" smd rect (at 2.854198 14.776958 270.0) (size 0.62992 2.249932) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" thru_hole circle (at -8.0645 10.174986 270.0) (size 1.868932 1.868932) (layers "*.Cu" "*.Mask") (drill 0.899922) (net 2 "NetJ1_6"))
  )
  (footprint "HDR1X6"
    (layer "F.Cu")
    (at 158.57237 97.844058 90.0)
    (property "Reference" "J1" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Header, 6-Pin" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "HDR1X6" (at 0 0 0) (layer "F.Fab"))
    (pad "5" smd rect (at -3.018028 -3.858514) (size 0.62992 2.249932) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" thru_hole circle (at -12.7 -0.0) (size 1.868932 1.868932) (layers "*.Cu" "*.Mask") (drill 0.899922) (net 2 "NetJ1_6"))
  )
  (footprint "SOD-123HE1_L3.0-W2.0-LS3.7-RD"
    (layer "F.Cu")
    (at 157.08012 113.527542)
    (property "Reference" "D3" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Schottky Diode" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "SOD-123HE1_L3.0-W2.0-LS3.7-RD" (at 0 0 0) (layer "F.Fab"))
    (pad "7" smd rect (at -2.366264 -15.205456 90.0) (size 0.62992 2.249932) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" thru_hole circle (at 1.49225 -8.063484 90.0) (size 1.868932 1.868932) (layers "*.Cu" "*.Mask") (drill 0.899922) (net 2 "NetJ1_6"))
  )
  (footprint "C0805"
    (layer "F.Cu")
    (at 155.39102 106.398524)
    (property "Reference" "C1" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Capacitor, X5R, ±10%, 6.3V" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "C0805" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -10.584688 -4.077208 90.0) (size 0.889 0.69977) (layers "F.Cu" "F.Paste" "F.Mask") (net 8 "NetLED1_C"))
    (pad "3" smd rect (at -7.737348 -6.806438 90.0) (size 0.62992 2.249932) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" thru_hole circle (at 3.18135 -6.014466 90.0) (size 1.868932 1.868932) (layers "*.Cu" "*.Mask") (drill 0.899922) (net 2 "NetJ1_6"))
  )
  (footprint "USB-A-PCB"
    (layer "F.Cu")
    (at 138.42763 105.166878 90.0)
    (property "Reference" "CN1" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "USB-A-PCB" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "USB-A-PCB" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 8.114792 9.226042) (size 0.62992 2.249932) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "1" thru_hole circle (at 7.32282 20.14474) (size 1.868932 1.868932) (layers "*.Cu" "*.Mask") (drill 0.899922) (net 2 "NetJ1_6"))
  )
  (footprint "R0603-NO"
    (layer "F.Cu")
    (at 153.076572 110.818632)
    (property "Reference" "R5" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Resistor, ±1%, 0.100W" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "R0603-NO" (at 0 0 0) (layer "F.Fab"))
    (pad "2" smd rect (at 5.70357 2.70891) (size 1.199896 1.399794) (layers "F.Cu" "F.Paste" "F.Mask") (net 3 "NetJ1_4"))
    (pad "1" smd rect (at -14.948916 -2.085086 90.0) (size 1.799844 7.999984) (layers "F.Cu" "F.Paste" "F.Mask") (net 5 "NetJ1_1"))
  )
  (footprint "R0603-NO"
    (layer "F.Cu")
    (at 151.574416 102.398024 180.0)
    (property "Reference" "R4" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Resistor, ±1%, 0.100W" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "R0603-NO" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.819912 -0.0 90.0) (size 0.889 0.69977) (layers "F.Cu" "F.Paste" "F.Mask") (net 7 "NetLED2_C"))
    (pad "C" smd rect (at -1.773174 -0.256794 90.0) (size 0.8001 0.8001) (layers "F.Cu" "F.Paste" "F.Mask") (net 11 "MISO"))
  )
  (footprint "R0603-NO"
    (layer "F.Cu")
    (at 145.626498 102.321316)
    (property "Reference" "R3" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Resistor, ±1%, 0.100W" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "R0603-NO" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 6.630162 8.497316 90.0) (size 0.889 0.69977) (layers "F.Cu" "F.Paste" "F.Mask") (net 6 "NetCN1_1"))
    (pad "C" smd rect (at 7.217156 9.891522) (size 0.8001 0.8001) (layers "F.Cu" "F.Paste" "F.Mask") (net 12 "VIN"))
  )
  (footprint "R0603-NO"
    (layer "F.Cu")
    (at 144.80811 97.852948)
    (property "Reference" "R2" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Resistor, ±1%, 0.100W" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "R0603-NO" (at 0 0 0) (layer "F.Fab"))
    (pad "2" smd rect (at 1.6383 4.468368 90.0) (size 0.889 0.69977) (layers "F.Cu" "F.Paste" "F.Mask") (net 8 "NetLED1_C"))
    (pad "3" smd rect (at -6.080506 6.26745 90.0) (size 1.199896 6.799834) (layers "F.Cu" "F.Paste" "F.Mask") (net 5 "NetJ1_1"))
    (pad "K" smd rect (at 2.90068 4.642358) (size 0.899922 0.799846) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "R0603-NO"
    (layer "F.Cu")
    (at 144.813444 96.472458)
    (property "Reference" "R1" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Resistor, ±1%, 0.100W" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "R0603-NO" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.819912 0.0 90.0) (size 0.889 0.69977) (layers "F.Cu" "F.Paste" "F.Mask") (net 10 "NetCN1_2"))
    (pad "1" smd rect (at -0.825246 1.38049 90.0) (size 0.889 0.69977) (layers "F.Cu" "F.Paste" "F.Mask") (net 9 "NetCN1_3"))
    (pad "2" smd rect (at -6.08584 9.721088 90.0) (size 1.199896 6.799834) (layers "F.Cu" "F.Paste" "F.Mask") (net 5 "NetJ1_1"))
    (pad "K" smd rect (at -1.388872 2.45618 90.0) (size 0.899922 0.799846) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "CHIP-LED0603"
    (layer "F.Cu")
    (at 154.097652 102.654818 270.0)
    (property "Reference" "LED2" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "SMD lamp beads" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "CHIP-LED0603" (at 0 0 0) (layer "F.Fab"))
    (pad "A" smd rect (at 0.0 -0.750062) (size 0.8001 0.8001) (layers "F.Cu" "F.Paste" "F.Mask") (net 11 "MISO"))
    (pad "6" smd rect (at -3.062732 -0.616204 180.0) (size 0.62992 2.249932) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "5" thru_hole circle (at 5.34924 -4.474718 180.0) (size 1.868932 1.868932) (layers "*.Cu" "*.Mask") (drill 0.899922) (net 2 "NetJ1_6"))
  )
  (footprint "CHIP-LED0603"
    (layer "F.Cu")
    (at 152.843654 112.9629)
    (property "Reference" "LED1" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "SMD lamp beads" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "CHIP-LED0603" (at 0 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 1.212088 -3.941318 270.0) (size 0.999998 2.499868) (layers "F.Cu" "F.Paste" "F.Mask") (net 14 "GND"))
    (pad "1" thru_hole circle (at -2.335784 0.136144 180.0) (size 1.868932 1.868932) (layers "*.Cu" "*.Mask") (drill 0.899922) (net 1 "D_N"))
  )
  (footprint "C0603"
    (layer "F.Cu")
    (at 156.497952 103.757178 90.0)
    (property "Reference" "C2" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Capacitor, X5R, ±10%, 6.3V" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "C0603" (at 0 0 0) (layer "F.Fab"))
    (pad "2" smd rect (at -0.704596 -2.44221 180.0) (size 0.999998 2.499868) (layers "F.Cu" "F.Paste" "F.Mask") (net 14 "GND"))
    (pad "1" smd rect (at -2.6162 -2.078228 270.0) (size 0.999998 1.399794) (layers "F.Cu" "F.Paste" "F.Mask") (net 4 "D_P"))
    (pad "2" smd rect (at 7.28472 -10.864342) (size 0.889 0.69977) (layers "F.Cu" "F.Paste" "F.Mask") (net 10 "NetCN1_2"))
    (pad "1" smd rect (at 0.790194 0.0 90.0) (size 1.09982 0.889) (layers "F.Cu" "F.Paste" "F.Mask") (net 13 "VCC5V"))
    (pad "1" smd rect (at -9.770364 -1.117854 270.0) (size 1.199896 1.399794) (layers "F.Cu" "F.Paste" "F.Mask") (net 3 "NetJ1_4"))
    (pad "A" smd rect (at -9.955784 -3.654298 270.0) (size 0.8001 0.8001) (layers "F.Cu" "F.Paste" "F.Mask") (net 12 "VIN"))
    (pad "8" smd rect (at 6.705092 -1.784096) (size 0.62992 2.249932) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" thru_hole circle (at -9.341866 -11.070082 90.0) (size 1.868932 1.868932) (layers "*.Cu" "*.Mask") (drill 0.899922) (net 1 "D_N"))
  )
  (footprint "TO252"
    (layer "F.Cu")
    (at 149.37503 106.741678 270.0)
    (property "Reference" "U1" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "5V Linear Regulator" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "TO252" (at 0 0 0) (layer "F.Fab"))
    (pad "3" smd rect (at -0.0 2.560066) (size 5.399786 5.599938) (layers "F.Cu" "F.Paste" "F.Mask") (net 14 "GND"))
    (pad "2" smd rect (at -0.3683 -6.990588 90.0) (size 0.999998 1.399794) (layers "F.Cu" "F.Paste" "F.Mask") (net 4 "D_P"))
    (pad "2" smd rect (at -4.343654 -1.379474) (size 0.889 0.69977) (layers "F.Cu" "F.Paste" "F.Mask") (net 7 "NetLED2_C"))
    (pad "2" smd rect (at 4.076954 -4.521708 180.0) (size 0.889 0.69977) (layers "F.Cu" "F.Paste" "F.Mask") (net 6 "NetCN1_1"))
    (pad "2" smd rect (at -2.19456 -7.122922 270.0) (size 1.09982 0.889) (layers "F.Cu" "F.Paste" "F.Mask") (net 13 "VCC5V"))
    (pad "4" smd rect (at -5.141468 11.247374 180.0) (size 1.799844 7.999984) (layers "F.Cu" "F.Paste" "F.Mask") (net 5 "NetJ1_1"))
    (pad "4" smd rect (at -5.879592 1.721358 180.0) (size 0.62992 2.249932) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "A" smd rect (at -4.246372 -0.333756 90.0) (size 0.899922 0.799846) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "A" smd rect (at -5.813044 5.950458 180.0) (size 0.899922 0.799846) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" thru_hole circle (at 6.357366 1.40716 270.0) (size 1.868932 1.868932) (layers "*.Cu" "*.Mask") (drill 0.899922) (net 1 "D_N"))
  )
  (footprint "SOIC8_208MIL"
    (layer "F.Cu")
    (at 151.183764 98.957086 90.0)
    (property "Reference" "U2" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "8KB 2.7V~5.5V AVR 512Byte 20MHz FLASH 6 SOIC-8-208mil Microcontrollers (MCU/MPU/SOC) ROHS" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "SOIC8_208MIL" (at 0 0 0) (layer "F.Fab"))
  )
  (footprint "SOD-323"
    (layer "F.Cu")
    (at 143.424572 99.928636 90.0)
    (property "Reference" "D1" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Independent Type 200mW 3.6V~3.8V 3.4V SOD-323 Zener Diodes ROHS" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "SOD-323" (at 0 0 0) (layer "F.Fab"))
  )
  (footprint "SOD-323"
    (layer "F.Cu")
    (at 148.708788 102.495306)
    (property "Reference" "D2" (at 0 -1.5 0) (layer "F.SilkS"))
    (property "Value" "Independent Type 200mW 3.6V~3.8V 3.4V SOD-323 Zener Diodes ROHS" (at 0 1.5 0) (layer "F.Fab"))
    (property "Footprint" "SOD-323" (at 0 0 0) (layer "F.Fab"))
  )
  (gr_line (start 156.917052 104.582424) (end 156.917052 102.982478) (layer "Edge.Cuts"))
  (gr_line (start 156.116952 104.582424) (end 156.917052 104.582424) (layer "Edge.Cuts"))
  (gr_line (start 156.116952 104.582424) (end 156.116952 102.982478) (layer "Edge.Cuts"))
  (gr_line (start 156.116952 102.982478) (end 156.917052 102.982478) (layer "Edge.Cuts"))
  (gr_line (start 156.348092 103.757178) (end 156.648066 103.757178) (layer "Edge.Cuts"))
  (gr_line (start 156.497952 103.907038) (end 156.497952 103.607064) (layer "Edge.Cuts"))
)
